Text for specification

Description
flexible copper busbar, tinned, insulated
10x 15.5 x 0.8
470 A, length 2 m
Accessories

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
Rated current (IEC):	470 A

power dissipation at full load of the item:	75,1 W

Material properties
Insulation:
	temperature withstand up to 105 °C
	self-extinguishing, V0 according to UL 94
	breakdown voltage 20 kV
	stretching 370 %

Miscellaneous 
Tin-plated Cu bars considerably reduce the effort of preparing the contact points.
The Cu busbars are effectively protected against aggressive media.

Brand 
Woehner or equivalent

Part No.
01091000