Text for specification

Description
QUADRON^®Panel
NH fuse-base 600 A, panel mounting, for PV 
incoming connection screw M10, outgoing connection to busbar 2x 40 x 10
size 2XL / 3L, 1P, with touch protection

Standards
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016

Electrical data
Rated current (IEC):	600 A
rated voltage (IEC) AC:	1000 V
rated voltage (IEC) DC:	1500 V

rated current (UL):	600 A
rated voltage (UL) DC:	1500 V

power dissipation at full load of the item:	13,8 W
rated surge voltage U_imp :	6 kV
short-circuit strength when protected by fuses:	50 kA

SCCR:	15 kA

Bei praxisgerechter Anordnung muss bezüglich Strombelastbarkeit, bezogen auf den Nennstrom der Sicherung, ein Reduktionsfaktor von 0,6 berücksichtigt werden.

for fuse links IEC 60269-6

Material properties
Main body:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free
Contacts:
	spring-loaded copper contacts, silver plated 
Connecting screws:
	screw M10, galvanized, chromized
Shock protection cover:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free

Miscellaneous 
For one or two internal busbars 40x10mm.
Busbar fully shock protected by the contact cover.
The shock protection is split into 2.

Brand 
Woehner or equivalent

Part No.
03293000