Text for specification

Description
CUSTO®60Classic
D-fuse base, busbar mounted, 57mm
screw-in gauge ring
E 33 / 3P
60Classic

Standards
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-3:2010 + A1:2013 + A2:2019

Electrical data
Rated current (IEC):	63 A
rated voltage (IEC) AC:	500 V
rated voltage (IEC) DC:	500 V

power dissipation at full load of the item:	10,0 W
rated surge voltage Uimp :	4 kV
max. permitted voltage (IEC) AC:	725 V
max. permitted voltage (IEC) DC:	630 V
short-circuit strength when protected by fuses:	50 kA

Contacting of the fuse links on the 	busbar via silvered copper plate

It can be used for branch circuits of the busbar system. The application as feeder of a busbars system is not accepted. 

as per DIN VDE 0636 Part 3011, also 690V

Brand 
Woehner or equivalent

Part No.
31442000