Text for specification

Description
EQUES®60Classic
busbar adapter 25 A
2 adjustable mounting rails
45 x 200, with screw terminals 6mm² from rear
60Classic

Standards
IEC 61439-1:2020

Approvals
CSA, UL

Electrical data
Rated current (IEC):	25 A
rated voltage (IEC) AC:	690 V

rated current (UL):	25 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	1,9 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV
max. permitted voltage (IEC) DC:	800 V

SCCR: 65 kA with any NKJH Comb. Motor Controller 25 A / 480 V AC, 65 kA with any NKJH Comb. Motor Controller 16 A / 480 V AC, 50 kA with any NKJH Comb. Motor Controller 32 A / 480 V AC, 30 kA with any NKJH Comb. Motor Controller 12,5 A / 600 V AC 

Material properties
Conductor insulation: 	temperature-resistant up to 105 °C

Brand 
Woehner or equivalent

Part No.
32436000