Text for specification

Description
EQUES®60Classic
busbar adapter 160 A, 3-pole
92 x 200
60Classic

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
Rated current (IEC):	160 A
rated voltage (IEC) AC:	690 V

rated current (UL):	160 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	17,7 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

Material properties
Conductor insulation: 	PVC, 	temperature-resistant up to 105 °C

Brand 
Woehner or equivalent

Part No.
32570000