Text for specification

Description
CAPUS^®Panel
switch disconnector with fuses, 3-pole
screw M10, red handle
size 2

Standards
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Approvals
IEC (CB)

Electrical data
Rated current (IEC):	400 A
rated voltage (IEC) AC:	690 V

AC-23B (690V)
AC-22B (690V)
AC-21B (690V)

power dissipation at full load of the item:	109,0 W

rated isolation voltage U_i AC:	1000 V
rated surge voltage U_imp :	8 kV

Terminal points
screw M10 :
Md 25 - 31 Nm

Brand 
Woehner or equivalent

Part No.
33361000