Text for specification

Description
CAPUS®Panel
switch-disconnector 3-pole + N
box terminal 16 - 50 mm² / AWG 6 - 1, yellow-red handle
100 A

Standards
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Approvals
UL

Electrical data
Rated current (IEC):	100 A
rated voltage (IEC) AC:	690 V

rated current (UL):	100 A
rated voltage (UL) AC:	600 V

AC-23 A (690 V / 63 A)
AC-23 A (415 V / 100 A)
AC-22 A (690 V / 100 A)
AC-21 A (690 V / 100 A)

power dissipation at full load of the item:	8,0 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	8 kV
rated making capacity:	3,5 kA

Terminal points
für Anwendungen nach IEC / EN :
16 - 50 mm² feindrähtig und rund mehrdrähtig
16 mm² rund eindrähtig
Md 3,5 Nm

50 mm² feindrährig mit Aderendhülse
Md 4,2 .... Nm ?

für Anwendungen nach UL / CSA :
AWG 6 - 1
31 lb-in

Miscellaneous 
lockable in 0-position with a padlock (max. 5 mm diameter) 

Brand 
Woehner or equivalent

Part No.
33893000A