Text for specification

Description
busbar connecting terminal 630 A
95 mm
60Classic

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
rated voltage (IEC) AC:	690 V

rated current (UL):	756 A

power dissipation at full load of the item:	1,3 W
current capacity (IEC) max.:	630 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  Ipk max.:	56,3 kA

SCCR:	25 kA

Brand 
Woehner or equivalent

Part No.
01141000