Text for specification

Description
clip-on screw connection, for cable lugs
M5
60Classic
100Energy
185mm-System
centre feed unit

Standards
IEC 61439-1:2011

Electrical data
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	0,5 W
current capacity (IEC) max.:	360 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  I_pk max.:	25,6 kA

Terminal points
Suitable for aluminium cables.
When using aluminium cables, observe the maintenance instructions.

Brand 
Woehner or equivalent

Part No.
01512000