Text for specification

Description
feed-through terminal 250 A
200 mm long, both sides screw M10

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	250 A
rated voltage (IEC) AC:	690 V
rated voltage (IEC) DC:	440 V

power dissipation at full load of the item:	2,7 W
max. permitted voltage (IEC) AC:	800 V
max. permitted voltage (IEC) DC:	800 V

Brand 
Woehner or equivalent

Part No.
03196000