Text for specification

Description
QUADRON^®Panel
NH fuse-base 250 A, panel mounting, for PV
incoming connection screw M10, outgoing connection to busbar 2x 30 x 10
size 1XL / 1P, with touch protection

Standards
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016

Approvals
UL

Electrical data
Rated current (IEC):	250 A
rated voltage (IEC) AC:	1000 V
rated voltage (IEC) DC:	1500 V

rated current (UL):	250 A
rated voltage (UL) DC:	1500 V

power dissipation at full load of the item:	5,5 W
rated surge voltage U_imp :	6 kV
short-circuit strength when protected by fuses:	50 kA

SCCR:	15 kA

for fuse links IEC 60269-6

Miscellaneous 
For one or two internal busbars 30x10mm.
Busbar fully shock protected by the contact cover.
The shock protection is split into 2.

Brand 
Woehner or equivalent

Part No.
03289000