Text for specification

Description
EQUES^®100Energy
busbar adapter 160 A
108 x 315
100Energy

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	160 A
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	17,8 W

rated isolation voltage U_i AC:	800 V
rated surge voltage U_imp :	6 kV

Brand 
Woehner or equivalent

Part No.
32001000