Text for specification

Description
EQUES^®60Classic
busbar adapter 32 A
1 adjustable mounting rail
45 x 200, without leads, with spring terminals 1.5 - 6 mm² from front
60Classic

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	32 A
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	2,5 W

rated isolation voltage U_i AC:	800 V
rated surge voltage U_imp :	6 kV
max. permitted voltage (IEC) DC:	800 V

Miscellaneous 
Free phase selection.
Click mechanism when pushing onto the busbar.

Brand 
Woehner or equivalent

Part No.
32486000