Text for specification

Description
CrossLink^®60Classic
spare part busbar adapter 160 A
busbar adapter base
60Classic

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	160 A
rated voltage (IEC) AC:	690 V
rated voltage (IEC) DC:	440 V

power dissipation at full load of the item:	11,9 W

rated isolation voltage U_i AC:	800 V
rated surge voltage U_imp :	6 kV
max. permitted voltage (IEC) AC:	725 V
max. permitted voltage (IEC) DC:	462 V

Miscellaneous 
Spare slot mounting, busbar cover
Simple and safe clicking into place and making contact
Busbar supports can be mounted above each other for flat busbars

Brand 
Woehner or equivalent

Part No.
32594000