Text for specification

Description
CAPUS®Panel
switch-disconnector 3-pole + N
box terminal 2.5 - 16 mm², graphite grey handle
63 A

Standards
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Electrical data
Rated current (IEC):	63 A
rated voltage (IEC) AC:	690 V

AC-23 A (690 V / 63 A)
AC-22 A (690 V / 63 A)
AC-21 A (690 V / 63 A)

power dissipation at full load of the item:	3,2 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	4 kV
rated making capacity:	2,1 kA

Miscellaneous 
lockable in 0-position with a padlock (max. 4 mm diameter) 

Brand 
Woehner or equivalent

Part No.
33825000A