Text for specification

Description
MOTUS®Panel
hybrid motor starter, 3-pole
direct and reversing starter 1.5 - 7.0 A / switch for resistive loads 1.5 - 9.0 A
with IO-Link interface

Standards
IEC 60947-1:2007 + A1:2010 + A2:2014
IEC 60947-4-2:2011
IEC 61508-1:2010
ISO 13849-1:2015

Approvals
UL

Electrical data
rated current (IEC):	9 A
rated voltage (IEC) AC:	500 V

rated current (UL):	7,6 A
rated voltage (UL) AC:	500 V

power dissipation at full load of the item:	12,0 W

rated isolation voltage Ui AC:	550 V
rated surge voltage Uimp :	6 kV

SCCR: 100 kA with JDDZ fuse Class J 175 A / 600 V AC  

Miscellaneous 
4 functions integrated:
Right contactor
Left contactor
Motor protection relay

Installed width only 22.5mm
30 million electrical switching operations

Brand 
Woehner or equivalent

Part No.
36126000A