Text for specification

Description
OMUS^®60Classic
hybrid switch, 3-pole or 1-pole switchable
switch for resistive loads 20.0 A, for applications UL
60Classic

Standards
IEC 60947-1:2007 + A1:2010 + A2:2014
IEC 60947-4-3:2014

Approvals
IEC (CB), UL

Electrical data
Rated current (IEC):	20 A
rated voltage (IEC) AC:	400 V

rated current (UL):	20 A
rated voltage (UL) AC:	480 V

power dissipation at full load of the item:	20,0 W

rated isolation voltage U_i AC:	500 V
rated surge voltage U_imp :	2,5 kV

Miscellaneous 
Up to 25A continuous current, including power monitoring
3 phase switching or independent phase switching is possible
Built-in functions for energy supply, fuse protection and switching
More than 30 million operating cycles through hybrid technology 

Brand 
Woehner or equivalent

Part No.
36158000A