Text for specification

Description
MIEZ
Power analyser for front panel installation
Measurement of current, voltage, power, energy and derived values
Analysis and monitoring of voltage and power quality

Standards
EN 61010-1:2011 + A1
EN 61010-2-030:2011 + O1 + Z1

Electrical data
rated voltage (IEC) AC:	24 V
rated voltage (IEC) DC:	24 V

power dissipation at full load of the item:	4,0 W
max. permitted voltage (IEC) AC:	50 V
max. permitted voltage (IEC) DC:	75 V

Brand 
Woehner or equivalent

Part No.
37010000A