Text for specification

Description
connection terminal, front connection
25 - 95 mm²
Accessories

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	225 A
rated voltage (IEC) AC:	400 V
rated surge voltage Uimp :	4 kV
max. permitted voltage (IEC) AC:	690 V
max. permitted voltage (IEC) DC:	600 V

Terminal points
25 - 90mm² round, solid and stranded
25 - 70mm² flexible with wire-end ferrule
Md 19Nm

Brand 
Woehner or equivalent

Part No.
01228000A