Text for specification

Description
D-fuse link 20 A
500 V, gG
E 27
Accessories

Standards
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-3:2010 + A1:2013 + A2:2019

Electrical data
Rated current (IEC):	20 A
rated voltage (IEC) AC:	500 V
rated voltage (IEC) DC:	500 V

power dissipation at full load of the item:	3.3 W

rated short-circuit breaking capacity AC:	50 kA
rated short-circuit breaking capacity DC:	8 kA

Brand 
Woehner or equivalent

Part No.
01675000