Text for specification

Description
CRITO®30Compact
connection set, 3-pole L1 + L2 + L3
10 - 120 mm²
30Compact 3P
30Compact 5P

Standards
IEC 61439-1:2020
IEC 60999-1:1999
IEC 60999-2:2003

Approvals
UL

Electrical data
Rated current (IEC):	250 A
rated voltage (IEC) AC:	690 V

rated current (UL):	200 A
rated voltage (UL) AC:	600 V
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  Ipk max.:	35.4 kA

SCCR:	18 kA

Brand 
Woehner or equivalent

Part No.
01370000