Text for specification

Description
busbar connecting terminal 1600 A
50 mm long
60Classic
185mm-System

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
rated voltage (IEC) AC:	690 V

rated current (UL):	1,400 A

power dissipation at full load of the item:	3.5 W
current capacity (IEC) max.:	1,600 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  Ipk max.:	72.7 kA

SCCR:	30 kA

Brand 
Woehner or equivalent

Part No.
01827000