Text for specification

Description
AMBUS^®Panel
holder for cylindrical fuses
10 x 38 / 3P/N
32 A / 690 V, N integrated

Standards
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Approvals
CCC

Electrical data
Rated current (IEC):	32 A
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	1.5 W

rated isolation voltage U_i AC:	690 V
rated surge voltage U_imp :	4 kV
max. permitted voltage (IEC) AC:	725 V

for fuse links as per IEC / EN 60269-2
with permitted rated power dissipations
up to max. 3W for gG/gL
up to max. 1.2W for aM

Miscellaneous 
large clamping range
holder for label

Brand 
Woehner or equivalent

Part No.
31274000A