Text for specification

Description
AMBUS®60Classic
busbar mounted fuse holder, with LED
for fuses Class CC, with LED 110 - 690 V AC / DC
Class CC / 3P
60Classic

Standards
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016, Fuse system J

Approvals
CSA, UL

Electrical data

rated current (UL):	30 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	1.8 W
short-circuit strength when protected by fuses:	200 kA

SCCR:	200 kA

Terminal points
nach IEC: Cu 1.5 … 6 mm2 (f, re)
nach UL /CSA: AWG 16 … AWG 10 (str)

Brand 
Woehner or equivalent

Part No.
31959000