Text for specification

Description
EQUES®60Classic
busbar adapter 250 A, 3-pole
105 x 240
60Classic

Standards
IEC 61439-1:2020

Approvals
CSA, UL

Electrical data
Rated current (IEC):	250 A
rated voltage (IEC) AC:	690 V

rated current (UL):	250 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	18.0 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

SCCR: 200 kA with 3VA61 150 A, 3VA62 250 A / 240 V AC, 50 kA with 3VA61 150 A, 3VA62 250 A / 600 V AC, 150 kA with 3VA61 150 A, 3VA62 250 A / 480 V AC 

Brand 
Woehner or equivalent

Part No.
32651000