Text for specification

Description
CRITO®CrossBoard
fastening module
at rear feeding

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
rated voltage (IEC) AC:	690 V

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV
max. permitted voltage (IEC) AC:	800 V
max. permitted voltage (IEC) DC:	800 V

Brand 
Woehner or equivalent

Part No.
01605000A