Text for specification

Description
QUADRON®Panel
holder for cylindrical fuses
Class J / 3P, terminal 150 mm²
200 A / 600 V

Standards
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016, Fuse system H

Approvals
UL

Electrical data

rated current (UL):	200 A
rated voltage (UL) AC:	600 V
rated voltage (UL) DC:	600 V

power dissipation at full load of the item:	13.0 W

SCCR:	200 kA

for Class J fuses 110 - 200A as per UL 248-8 (41x146)

Terminal points
AWG 2 - MCM 300 stranded, equivalent to 33,6 - 152mm²

Material properties
Main body:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free
Handle:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 200,
	halogen-free

Brand 
Woehner or equivalent

Part No.
33409000