Text for specification

Descripción
CRITO®60Classic
placa de bornes de conexión, 3 polos
lam. Cu. 20 - 32 x 3 - 15
60Classic

Normas
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

datos eléctricos
intensidad de corriente nominal (IEC):	550 A
tensión nominal (IEC) AC:	690 V
máxima intensidad de corriente (IEC):	800 A
tensión máxima (IEC) AC:	1000 V
tensión máxima (IEC) DC:	1500 V

resistencia a corriente de pico Ipk máx. :	63.1 kA

puntos de apriete
plet. flex. desde 3 x 20 x 1 hasta 10 x 32 x 1

cualidad de materiales
Cuerpo principal:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 200,
	halogen-free
Cubierta:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 200,
	halogen-free

Terminals: 	galvanised steel, chromited screw: 	hexagon socket screw, galvanised, chromited, thrust piece 	brass, nickel-plated

Miscellaneous 
also rigid copper busbars can be connected if they are installed without mechnical tension 

Brand 
Woehner or equivalent

Part No.
01753000