Text for specification

Descripción
SECUR®Panel
seccionador para fusibles D0 de hasta 63 A
con LED
1P

Normas
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

homologaciónes
VDE

datos eléctricos
intensidad de corriente nominal (IEC):	63 A
tensión nominal (IEC) AC:	400 V
tensión nominal (IEC) DC:	65 V

AC-22B (400V)

 DC-22B (65 V)

power dissipation at full load of the item:	2.6 W

tensión nominal de aislamiento Ui AC:	500 V
tensión de pico Uimp:	6 kV

for fuse links and gauge rings as per DIN VDE 0636-3 IEC / HD 60269-3
utilisation category as per VDE 0638: AC-22 (400V)

The function of isolation between incoming and outgoing contacts is provided by the opening of the switching mechanism as required in the standard.

There is a transfer of the potential from the busbars, through the LED units, to the terminals  when the fuse links are removed and the switching mechanismn is closed. 

Miscellaneous 
Double function terminal
any feed direction
captive fuse-carrier
sealable operation

Brand 
Woehner or equivalent

Part No.
31556000A