Text for specification

Descripción
actuador giratorio de acoplamiento a puerta
Accessories

Normas
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

datos eléctricos

Miscellaneous 
lockable in 0-position with 3 padlocks (max. 6 mm diameter) door interlock in I-position door interlock in I-position defeatable with a tool 

Brand 
Woehner or equivalent

Part No.
33670000A