Text for specification

Descripción
CRITO^®CrossBoard
módulo de conexión
con bornes elásticos integrados, 1,5-16 mm², AWG 14-6
3 polos

Normas
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

homologaciónes
IEC (CB), UL

datos eléctricos
intensidad de corriente nominal (IEC):	63 A
tensión nominal (IEC) AC:	690 V

intensidad de corriente nominal (UL):	48 A
tensión nominal (UL) AC:	600 V

power dissipation at full load of the item:	4.6 W
máxima intensidad de corriente (IEC):	80 A

tensión nominal de aislamiento Ui AC:	800 V
tensión máxima (IEC) AC:	800 V
tensión máxima (IEC) DC:	800 V

resistencia a corriente de pico Ipk máx. :	10 kA

puntos de apriete
For leads per IEC :
1.5 - 16 mm² round stranded and finely stranded without wire-end ferrule
1.5 - 16 mm² finely stranded with wire-end ferrule*
1.5 - 10 mm² finely stranded with wire-end ferrule 
1.5 - 10 mm² round solid 

* Recommendation: 16 mm² crimped with Rittal crimping pliers for wire-end ferrules WM-Crimp, Weidmüller crimping tool PZ 16 or Phoenix Contact crimping pliers Crimpfox 25R

for leads per UL:
Cu AWG 14 - 6
Class B (UL486E)

Brand 
Woehner or equivalent

Part No.
01592000A