Text for specification

Descripción
MOTUS®60Classic
Arrancador híbrido de motor, 3 polos
0,075 - 0,6 A Arrancador directo e inversor de giro / interruptor para cargas resistivas
60Classic

Normas
EN 60947-1:2015
EN 60947-4-2:2012
EN 61439-1:2012
EN 50581:2012
EN ISO 13849-1:2015

homologaciónes
UL, CCC

datos eléctricos
intensidad de corriente nominal (IEC):	0.6 A
tensión nominal (IEC) AC:	500 V

intensidad de corriente nominal (UL):	0.6 A
tensión nominal (UL) AC:	500 V

power dissipation at full load of the item:	2.8 W

tensión nominal de aislamiento Ui AC:	500 V
tensión de pico Uimp:	6 kV

SCCR: 100 kA with JDDZ fuse Class J 400 A / 600 V AC  

puntos de apriete
Screw terminals (solid round, flexible, flexible with wire-end ferrule) 
0.14 - 2.5mm² / 0.5 - 0.6Nm
The cable outlet is provided with a pluggable terminal

Miscellaneous 
4 functions integrated:
Right contactor
Left contactor
Motor protection relay
EMERGENCY STOP protection up to category 3

Installed width only 22.5mm
30 million electrical switching operations

Brand 
Woehner or equivalent

Part No.
36102000B