Text for specification

Descripción
QUADRON^®Panel
parte inferior de base NH de 250 A, montaje en superficie, para sistemas fotovoltaicos
tornillo de borne de entrada M10, conector de salida al embarrado de 2 x 30 x 10, para el montaje integrado de transformadores de corriente de tipo LEM HTA
talla 1XL/1P, con protección contra contacto

Normas
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016

datos eléctricos
intensidad de corriente nominal (IEC):	250 A
tensión nominal (IEC) AC:	1000 V
tensión nominal (IEC) DC:	1500 V

power dissipation at full load of the item:	5,5 W
tensión de pico Uimp:	6 kV
corriente de cortocircuito cuando se protege por fusibles:	50 kA

for fuse links IEC 60269-6

puntos de apriete
Connection screws for busbars: Hexagonal screw M10, length across flats 16, tightening torque 30Nm
connection width 25mm 
fastening to mounting plate: 2x 10.5mm hole, intended for hexagonal screw M10, tightening torque 5Nm

cualidad de materiales
Cuerpo principal:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free
Contactos:
	spring-loaded copper contacts, silver plated 
Tornillos de conexión:
	screw M10, galvanized, chromized
Protección contra contacto:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free

Miscellaneous 
For one or two internal busbars 30x10mm.
Busbar fully shock protected by the contact cover.
The shock protection is split into 2.

Brand 
Woehner or equivalent

Part No.
03288000