Text for specification

Descripción
AMBUS®Panel
soporte para fusibles cilíndricos
10 x 38 / 3P/N
32 A/690 V, N integrado

Normas
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

homologaciónes
CCC

datos eléctricos
intensidad de corriente nominal (IEC):	32 A
tensión nominal (IEC) AC:	690 V

power dissipation at full load of the item:	1,5 W

tensión nominal de aislamiento Ui AC:	690 V
tensión de pico Uimp:	4 kV
tensión máxima (IEC) AC:	725 V

for fuse links as per IEC / EN 60269-2
with permitted rated power dissipations
up to max. 3W for gG/gL
up to max. 1.2W for aM

cualidad de materiales
Cuerpo principal:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free
Soporte de fusibles:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free
	
Tornillos de conexión:
	screw +/- (PZ2), galvanized, chromized 

Miscellaneous 
large clamping range
holder for label

Brand 
Woehner or equivalent

Part No.
31274000A