Text for specification

Descripción
EQUES®185Power
adaptador para embarrado de 1400 A
300 x 652, conexión inferior, conexión por brida, fase cambiada 
185Power

The 185Power is an innovative busbar system for energy distribution coming with busbar system, connection rails and modules as feeders, busbar connectors, NH in-line fuse-switch-disconnectors, NH switch-disconnector-fuses and adapters for circuit breakers.

 By using Crosslink touch-safe protection modules, it is possible to build a touch-protected 185mm busbar system.

 Crosslink touch-safe protection cover with protection class IP2X front.
 Crosslink touch-safe protection cover with additional front cover enhance protection class to IP4X front.

 All system components can be mounted safely, easily and quickly on the Crosslink touch-safe protection modules using terminal clamps.

The busbar system comes with copper busbars of 30mm, 40mm, 60mm, 80mm, 100mm, 120mm x 10mm. For selected application set up’s, short circuit capabilities are proven by tests. The achievable maximum ratings are rated peak withstand current Ipk max. 105kA, rated short-time withstand current Icw max. 50kA at 1 second. 

Normas
IEC 61439-1:2011

homologaciónes
UL

datos eléctricos
intensidad de corriente nominal (IEC):	1.400 A
tensión nominal (IEC) AC:	690 V
tensión nominal (IEC) DC:	800 V

intensidad de corriente nominal (UL):	1.200 A
tensión nominal (UL) AC:	1000 V

power dissipation at full load of the item:	417,0 W

tensión nominal de aislamiento Ui AC:	1000 V
tensión de pico Uimp:	12 kV

resistencia a corriente de pico Ipk máx. :	106 kA

mit Schneider Electric NS1600 bis 1400A einsetzbar!

Brand 
Woehner or equivalent

Part No.
32718000A