Text for specification

Descripción
EQUES 185Power
adaptador para embarrado de 1440 A
300 x 652, conexión frontal, conexión atornillada 
185Power

The 185Power is an innovative busbar system for energy distribution coming with busbar system, connection rails and modules as feeders, busbar connectors, NH in-line fuse-switch-disconnectors, NH switch-disconnector-fuses and adapters for circuit breakers.

 By using Crosslink touch-safe protection modules, it is possible to build a touch-protected 185mm busbar system.

 Crosslink touch-safe protection cover with protection class IP2X front.
 Crosslink touch-safe protection cover with additional front cover enhance protection class to IP4X front.

 All system components can be mounted safely, easily and quickly on the Crosslink touch-safe protection modules using terminal clamps.

The busbar system comes with copper busbars of 30mm, 40mm, 60mm, 80mm, 100mm, 120mm x 10mm. For selected application set up’s, short circuit capabilities are proven by tests. The achievable maximum ratings are rated peak withstand current Ipk max. 105kA, rated short-time withstand current Icw max. 50kA at 1 second. 

Normas
IEC 61439-1:2020

homologaciónes
UL

datos eléctricos
intensidad de corriente nominal (IEC):	1.440 A
tensión nominal (IEC) AC:	800 V
tensión nominal (IEC) DC:	800 V

intensidad de corriente nominal (UL):	1.200 A
tensión nominal (UL) AC:	1000 V

power dissipation at full load of the item:	548,0 W

tensión nominal de aislamiento Ui AC:	1000 V
tensión de pico Uimp:	12 kV

resistencia a corriente de pico Ipk máx. :	106 kA

mit Legrand DPX³ 1600 oder GE FK1600, nur geeignet für Verbindung oben, bis 1440A einsetzbar!

Brand 
Woehner or equivalent

Part No.
32809000A