Text for specification

Descripción
BROOME10®30Compact
fuente de alimentación 10 A
400 V AC / 24 V DC, con bornes por presión
30Compact 3P

Normas
IEC 61010-1:2010
IEC 61010-2-201:2013

homologaciónes
IEC (CB), UL

datos eléctricos
tensión nominal (IEC) AC:	480 V
tensión nominal (UL) AC:	480 V

tensión nominal de aislamiento Ui AC:	800 V
tensión de pico Uimp:	6 kV

Further technical data: 

max. input inrush current: 1,5 A

periodic and random deviation: 50 mVpp

hold-up time (typical): 20 ms

input / output separation: SELV / PELV

output overvoltage protection: max. 32 V dc

parallel installation to increase the power: 
up to 30 A without additional protection
for more than 30 A each output has to be protected by a fuse 16 A

serial installation to increase the voltage: 
up to 72 V dc (note: Ab at 60 V dc and more: no SELV)

puntos de apriete
Push-in-Klemme:
IEC: 
bis max. 2,5 mm² re, f
bis max. 1,5 mm² f+AE

UL:
AWG 24 - AWG 12

Miscellaneous 
efficiency of 95% permits an intallation width of 45 mm
self-protected at short-circuit with intelligent re-start
no pre-fuse needed
overvoltage capacity up to 6 kV

Brand 
Woehner or equivalent

Part No.
36201000A