Text for specification

Descripción
QUADRON®60Classic
portafusibles sobre barras, Class J, conexión superior / inferior
para fusibles Class J de 225-400 A (54x181)
3P, con borne-brida
60Classic

Normas
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016, Fuse system H

homologaciónes
CSA, UL

datos eléctricos

intensidad de corriente nominal (UL):	400 A
tensión nominal (UL) AC:	600 V
tensión nominal (UL) DC:	600 V

power dissipation at full load of the item:	46,8 W

SCCR:	65 kA

puntos de apriete
tunnel terminal with hole of 23,0 mm diameter

acc. to IEC / EN :
16 - 240 (300) mm²
flexible cables, directly or with wire-end ferrule, 
solid and stranded round cables, 
Md 38 - 40 Nm

(flexible cables of maximum cross-section may not fit when using wire-end ferrule)

acc. to UL :
AWG 4 - MCM 600
stranded cables Class B acc. to UL 486E
336 - 355 lb.in.

cualidad de materiales
Cuerpo principal:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 200,
	halogen-free
Protección contra contacto:
	temperature stability 125°C,
	fire behaviour UL 94 HB,
	creepage resistance CTI 200,
	halogen-free 
Tornillos de conexión:
	screw M12, galvanized, chromized

Miscellaneous 
the product is based on the UL approval in category IZLT2 also listed in category NMTR (file E123577)

Brand 
Woehner or equivalent

Part No.
33311000