Text for specification

Descripción
MOTUS®30Compact
Arrancador híbrido de motor, 3 polos
0,18 - 3 A Arrancador directo e inversor de giro con IO-Link / interruptor para cargas resistivas
con IO-Link interface
30Compact 3P

Normas
IEC 60947-1:2007 + A1:2010 + A2:2014
IEC 60947-4-2:2011
IEC 61508-1:2010
ISO 13849-1:2015

homologaciónes
UL

datos eléctricos
intensidad de corriente nominal (IEC):	3 A
tensión nominal (IEC) AC:	500 V

intensidad de corriente nominal (UL):	3 A
tensión nominal (UL) AC:	500 V

power dissipation at full load of the item:	6,0 W

tensión nominal de aislamiento Ui AC:	550 V
tensión de pico Uimp:	6 kV

SCCR: 100 kA with JDDZ fuse Class J 175 A / 600 V AC  

puntos de apriete
Screw terminals (solid round, flexible, flexible with wire-end ferrule) 
0.14 - 2.5mm² / 0.5 - 0.6Nm
The cable outlet is provided with a pluggable terminal

cualidad de materiales
Caja:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free

Miscellaneous 
4 functions integrated:
Right contactor
Left contactor
Motor protection relay

Installed width only 22.5mm
30 million electrical switching operations

Brand 
Woehner or equivalent

Part No.
36124000A