Text for specification

Descripción
pletina flexible, lisa, aislada
4x 24 x 1
438 A, longitud 2 m
Accessories

Normas
IEC 61439-1:2011

homologaciónes
UL

datos eléctricos
intensidad de corriente nominal (IEC):	438 A

power dissipation at full load of the item:	84,2 W

Miscellaneous 
The laminated Cu busbars considerably reduce the effort of connecting busbars. The bending devices required for solid copper busbars are unnecessary. The 2mm-thick insulation means that no additional covering is required.

Brand 
Woehner or equivalent

Part No.
01253000