Text for specification

Désignation
support de jeu de barres
3 pôles, avec bornes intégrées de 1,5 à 16 mm²
60Classic

Normes
IEC 61439-1:2011

Charactéristiques électriques
Courant assigné (IEC):	63 A
Tension assignée (IEC) CA:	690 V

power dissipation at full load of the item:	0,8 W
current capacity (IEC) max.:	80 A

rated isolation voltage Ui AC:	800 V
Tension assignée de tenue aux chocs Uimp:	6 kV

Current capacity of the clamping point 80A
short-circuit withstand rating:
surge current strength &gt; 30kA at busbar support separation of 550mm
surge current strength &gt; 50kA at busbar support separation of 250mm
further values in the short-circuit withstand rating diagram

Charactéristiques des matériaux
Embase:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free
Vis:
	screw +/- (PZ2), galvanized, chromized 
Couvercle:
	tenue en température 125°C, 
	auto-extinguible conf. à l'UL 94,
	tenue au courant de fuite CTI 600

Miscellaneous 
Connection busbar support with integrated terminals for feeding or tapping the busbar
with internal screw holes, can also be used as centre support.

Brand 
Woehner or equivalent

Référence
01484000