Text for specification

Désignation
CRITO®
bornes à pince
Cu / Al 95 - 185 mm²
60Classic
100Energy
185mm-System
centre feed unit

Normes
IEC 61439-1:2020
IEC 60999-1:1999
IEC 60999-2:2003

Approbations
UL

Charactéristiques électriques
Courant assigné (IEC):	300 A
Tension assignée (IEC) CA:	690 V

rated current (UL):	310 A
rated voltage (UL) AC:	600 V
current capacity (IEC) max.:	500 A
Tension maximale IEC CA:	1000 V
Tension maximale IEC CC:	1500 V

rated peak withstand current  Ipk max.:	55,8 kA

Icc:	25 kA

Points de raccordement
for applications acc. to IEC / EN :
Cu or Al 95 - 185 mm² stranded round cables and stranded sectored cables
Cu also flexible cables, directly,

for applications acc. to UL / CSA :
Cu 95 - 185 mm² / AWG 3/0 - MCM 350
Suitable for aluminium cables.
When using aluminium cables, observe the maintenance instructions.

Miscellaneous 
Terminal with captive clamp screws, conductor can be overlapped, indication of nominal cross-section and tightening torque noted on the terminal, contact between conductor and busbar via cable bed.

Brand 
Woehner or equivalent

Référence
01318000