Text for specification

Désignation
CRITO^®CrossBoard
bornier de raccordement
avec bornes à ressort intégrées 1.5 - 16 mm², AWG 14 - 6
3 pôles

Normes
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Approbations
IEC (CB), UL

Charactéristiques électriques
Courant assigné (IEC):	63 A
Tension assignée (IEC) CA:	690 V

rated current (UL):	48 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	4,6 W
current capacity (IEC) max.:	80 A

rated isolation voltage U_i AC:	800 V
Tension maximale IEC CA:	800 V
Tension maximale IEC CC:	800 V

rated peak withstand current  I_pk max.:	10 kA

Points de raccordement
For leads per IEC :
1.5 - 16 mm² round stranded and finely stranded without wire-end ferrule
1.5 - 16 mm² finely stranded with wire-end ferrule*
1.5 - 10 mm² finely stranded with wire-end ferrule 
1.5 - 10 mm² round solid 

* Recommendation: 16 mm² crimped with Rittal crimping pliers for wire-end ferrules WM-Crimp, Weidmüller crimping tool PZ 16 or Phoenix Contact crimping pliers Crimpfox 25R

for leads per UL:
Cu AWG 14 - 6
Class B (UL486E)

Brand 
Woehner or equivalent

Référence
01592000A