Text for specification

Désignation
SECUR®Panel
sectionneur à fusibles D0 jusqu'à 63 A
avec LED
1P

Normes
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Approbations
VDE

Charactéristiques électriques
Courant assigné (IEC):	63 A
Tension assignée (IEC) CA:	400 V
Tension assignée (IEC) CC:	65 V

AC-22B (400V)

DC-22B (65 V)

power dissipation at full load of the item:	2,6 W

rated isolation voltage Ui AC:	500 V
Tension assignée de tenue aux chocs Uimp:	6 kV

for fuse links and gauge rings as per DIN VDE 0636-3 IEC / HD 60269-3
utilisation category as per VDE 0638: AC-22 (400V)

The function of isolation between incoming and outgoing contacts is provided by the opening of the switching mechanism as required in the standard.

There is a transfer of the potential from the busbars, through the LED units, to the terminals  when the fuse links are removed and the switching mechanismn is closed. 

Miscellaneous 
Double function terminal
any feed direction
captive fuse-carrier
sealable operation

Brand 
Woehner or equivalent

Référence
31556000A