Text for specification

Désignation
CRITO^®
bornes à pince
lam. Cu. 20x3 ... 32x15
60Classic
100Energy
185mm-System
centre feed unit

Normes
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Approbations
UL

Charactéristiques électriques
Courant assigné (IEC):	500 A
Tension assignée (IEC) CA:	690 V

rated current (UL):	800 A
rated voltage (UL) AC:	600 V
Tenue au courant avec alimentation au milieu:	750 A
current capacity (IEC) max.:	750 A
Tension maximale IEC CA:	1000 V
Tension maximale IEC CC:	1500 V

Icc:	25 kA

Points de raccordement
la. Cu de 3 x 20 x 1 à 10 x 24 x 1

Charactéristiques des matériaux
Vis de raccordement:
	Set screw M16, Allan key size 8
Corps de borne:
	steel, galvanized and chromized
cable base:
	brass, tin plated

Terminal body: 	galvanised steel, chromited screw: 	hexagonal socket screw M16 x 1.5 (S8), galvanised, chromited

Miscellaneous 
Terminal with captive clamping screws, conductor can be overlapped, indication of nominal cross-section and tightening torque noted on the terminal. Contact between conductor and busbar via contact block.

Brand 
Woehner or equivalent

Référence
01319000