Text for specification

Désignation
MOTUS^®60Classic
démarreur moteur hybride 3 pôles
démareur direct inverse de 0,075 - 0,6 A / contacteur de charge résistive de 0,075- 0,6 A
60Classic

Normes
EN 60947-1:2015
EN 60947-4-2:2012
EN 61439-1:2012
EN 50581:2012
EN ISO 13849-1:2015

Approbations
UL, CCC

Charactéristiques électriques
Courant assigné (IEC):	0,6 A
Tension assignée (IEC) CA:	500 V

rated current (UL):	0,6 A
rated voltage (UL) AC:	500 V

power dissipation at full load of the item:	2,8 W

rated isolation voltage U_i AC:	500 V
Tension assignée de tenue aux chocs Uimp:	6 kV

SCCR: 100 kA with JDDZ fuse Class J 400 A / 600 V AC  

Points de raccordement
Screw terminals (solid round, flexible, flexible with wire-end ferrule) 
0.14 - 2.5mm² / 0.5 - 0.6Nm
The cable outlet is provided with a pluggable terminal

Charactéristiques des matériaux
Boîtier:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free

Miscellaneous 
4 functions integrated:
Right contactor
Left contactor
Motor protection relay
EMERGENCY STOP protection up to category 3

Installed width only 22.5mm
30 million electrical switching operations

Brand 
Woehner or equivalent

Référence
36102000B