Text for specification

Désignation
MOTUS^®Panel
démarreur moteur hybride 3 pôles
démareur direct inverse de 0,18 - 2,4 A / contacteur de charge résistive de 0,18 - 2,4 A

Normes
EN 60947-1:2015
EN 60947-4-2:2012
EN 61439-1:2012
EN 50581:2012
EN ISO 13849-1:2015

Approbations
UL, CCC

Charactéristiques électriques
Courant assigné (IEC):	2,4 A
Tension assignée (IEC) CA:	500 V

rated current (UL):	2 A
rated voltage (UL) AC:	500 V

power dissipation at full load of the item:	5,5 W

rated isolation voltage U_i AC:	500 V
Tension assignée de tenue aux chocs Uimp:	6 kV

SCCR: 100 kA with JDDZ fuse Class J 175 A / 600 V AC  

Points de raccordement
Screw terminals (solid round, flexible, flexible with wire-end ferrule) 
0.14 - 2.5mm² / 0.5 - 0.6Nm
The cable outlet is provided with a pluggable terminal

Miscellaneous 
4 functions integrated:
Right contactor
Left contactor
Motor protection relay
EMERGENCY STOP protection up to category 3

Installed width only 22.5mm
30 million electrical switching operations

Brand 
Woehner or equivalent

Référence
36103000B