Text for specification

Désignation
CRITO^®
borne de raccordement universelle
4 - 35 mm², AWG 12 - 2
30Compact 3P
60Classic
100Energy
185mm-System

Normes
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Approbations
CSA, UL

Charactéristiques électriques
Courant assigné (IEC):	115 A
Tension assignée (IEC) CA:	690 V

rated current (UL):	115 A
rated voltage (UL) AC:	600 V
current capacity (IEC) max.:	270 A
Tension maximale IEC CA:	1000 V
Tension maximale IEC CC:	1500 V

rated peak withstand current  I_pk max.:	34,9 kA

Points de raccordement
4 - 35 mm² / AWG 10 - AWG 2 
câble souple, direct ou avec embout, 
rigide ou rond multi-brins, 
la. Cu 3 x 9 x 0,8 ou 6 x 9 x 0,8

(câble souple de section maxi ne convient pas si équipé d'embout)

Charactéristiques des matériaux
Vis de raccordement:
	screw +/- (PZ3), galvanized, chromized 
Corps de borne:
	steel, galvanized and chromized
Retaining spring:
	corrosion-resistant spring steel

Miscellaneous 
Terminal with integrated holding spring, captive clamping screw and opened terminal space.
Indication of nominal cross-section and tightening torque noted on the terminal.

Brand 
Woehner or equivalent

Référence
01290000