Text for specification

Désignation
CRITO®60Classic
plaque bornier, 3 pôles
95 - 185 mm²
60Classic

Normes
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Charactéristiques électriques
Courant assigné (IEC):	350 A
Tension assignée (IEC) CA:	690 V
current capacity (IEC) max.:	460 A
Tension maximale IEC CA:	1000 V
Tension maximale IEC CC:	1500 V

rated peak withstand current  Ipk max.:	55,8 kA

Points de raccordement
für Anwendungen nach IEC / EN :
Cu und Al 95 - 185 mm² Rundleiter mehrdrähtig und Sektorleiter mehrdrähtig
Cu auch feindrähtig, direkt geklemmt

for applications acc. to IEC / EN:
Cu or Al 95 - 185mm², round stranded or sector-shaped stranded cables
also fine stranded Cu cables (direct clamping)   

Suitable for aluminium cables.
When using aluminium cables, observe the maintenance instructions.

Miscellaneous 
Terminals with captive clamping screws
Conductor can be overlapped
Indication of nominal cross-section and tightening torque noted on the terminals.

Brand 
Woehner or equivalent

Référence
01199000