Text for specification

Désignation
rail de cuivre en lamelles, dénudé, isolé
10x 15.5 x 0.8
470 A, longueur 2 m
Accessories

Normes
IEC 61439-1:2011

Approbations
UL

Charactéristiques électriques
Courant assigné (IEC):	470 A

power dissipation at full load of the item:	75,1 W

Miscellaneous 
The laminated Cu busbars considerably reduce the effort of connecting busbars. The bending devices required for solid copper busbars are unnecessary. The 2mm-thick insulation means that no additional covering is required.

Brand 
Woehner or equivalent

Référence
01583000